**Protocol to Use LSM 880**

* [Locate] to choose focus area
* Use FCF AS – setting (oil-1 drop)
* Adjust focus Hexagon (Brightest in the center)
* White value >6000
* 20sec to stabilize the CO2 5% (For live cells)